;General field properties
[sr_psy_antenna@def]
mute_sound_threshold = 1
postprocess = pas_b400_acidic.ppe
eff_intensity = 100
hit_intensity = 1.05
no_mumble = true
no_static = true
hit_type = chemical
hit_freq = 25
